|  |  |
| --- | --- |
| Model | EC-MW2003 |
| Camera type | HD Waterproof IR Mobile Camera |
| Image Sensor |      2.0 megapixel CMOS Sony IMX307 Sensor |
| Effective Pixels | PAL:1920x1080@25fps NTSC:1920x1080@30fps |
| Resolution | 1920x1080 |
| IR-LED | 10pcs  Ф5mm IR Leds |
| Illuminate Distance | 20m IR Distance |
| Day/Night | IR-CUT filter |
| Min.Illumination | Color 0.1Lux/F1.2, B/W 0.01Lux/F1.2 |
| Electronic Shutter | 4/25-1/45,000s |
| Lens | 2.8 mm Lens |
| Lens Mount | M12 |
| Video output | 1CH 4IN1 AHD/TVI/CVI/Analog Video output |
| Work environment | -10℃~60℃90％RH |
| Power supply | DC 12V±10% |
| BLC | Auto BLC |
| White Balance | Auto White Balance |
| Max transmission distance | common 75-3 lines can be up to 300 m |
| other function | D-WDR,3D-DNR |
| Waterproof Criterion | IP66 |